Lang{
"Anyka_USB_Burn_Tool",
"Update Mode",
"File(&F)",
"Import File(&I)",
"Export File(&O)",
"Settings(&S)",
"Burn Settings",
"Change Password",
"View(&V)",
"Language",
"COM Window",
"Tool(&T)",
"Create SPI NOR Flash Image Offline(&I)",
"Read Back SPI NOR Flash Image(&S)",
"Read Back BIN(&B)",
"Configure Files(&C)",
"Help(&H)",
"About Anyka_USB_Burn Tool(&A)",
"Start",
"Burn Settings",
"Import",
"Export",
"Low-level Formatting",
"Status",
"Item",
"Progress",
"Status Description",
"Timer",
"Serial Number",
"MAC Address",
"Device",
"Current Link",
"Available Link",
"Burn Count",
"Total Pass",
"Total Fail",
"Clear",
"Burn Information",
"USB Device",
"Udisk",
"Auto Burn",
"Udisk Burn",
"Online Image creation (only device0 & only once)",
"No fixed burning channels",
"Udisk massboot",
"Producer",
"Researcher",
"Please enter the User and Password:",
"User",
"Password",
"Change Password",
"User",
"Old Password",
"New Password",
"Confirm Password",
"Wrong password!",
"Those passwords didn't match!",
"Success!You've changed your password.",
"Ready",
"Udisk update is Ready",
"Start burn",
"Start to set RAM parameter",
"Failed to set RAM parameter",
"Start to set registers",
"Failed to set registers",
"Failed to get registers",
"Success!You've set registers",
"Start to initialize USB",
"Failed to initialize USB",
"Completion",
"Start to test RAM",
"Failed to test RAM",
"Begin to download producer",
"Failed to download producer",
"Failed to connect USB after download producer",
"Download producer time out",
"Success!You've downloaded producer",
"Partition info is null",
"Failed to get medium data info",
"Failed to get free block info",
"Start to create partition",
"Failed to create partition",
"Failed to create medium",
"Start to test",
"Failed to test",
"Begin to get SPI NAND Flash chip ID",
"Failed to get SPI NAND Flash chip ID",
"Begin to set SPI NAND Flash chip parameter",
"Failed to set SPI NAND Flash chip parameter",
"The SPI parameter is not in burn tool list",
"Failed to send the extended parameter or set boot partition size",
"Begin to get SPI NOR Flash chip ID",
"Failed to get SPI NOR Flash chip ID",
"Begin to set SPI NOR Flash chip parameters",
"Failed to set SPI NOR Flash chip parameters",
"Begin to erase",
"Failed to erase",
"Begin to format",
"Failed to format",
"Begin to download file",
"Failed to download file",
"Start to get activation file",
"Failed to get activation file",
"Project ",
"Channel Number",
"Platform",
"Carrier burn for no USB chip.",
"Open COM",
"COM Number ",
"COM Base",
"Baud Rate",
"Configure Command Line",
"Address",
"Data",
"Burn MAC Address",
"Force to write MAC address.",
"Reset current MAC.",
"Start Address(0x)",
"End Address(0x)",
"Burn Serial Number",
"Force to write serial number.",
"Start prefix(0x)",
"End prefix(0x)",
"Serial Number",
"Burn Bluetooth address.",
"Force to burn Bluetooth address.",
"Bluetooth Start Address",
"Bluetooth End Address",
"Browse",
"Producer",
"Boot ",
"Boot(37L) ",
"BIOS",
"Burn file to system partition",
"Burn BIN",
"System Partition Image of Burn File",
"Burn SPI NOR Flash Image",
"No.",
"Compare Or Not?",
"YES",
"NO",
"PC Path",
"Download File",
"Download Directory",
"Download Path",
"Start Address",
"End Address",
"Backup Start Address",
"Backup End Address",
"Drive letter",
"Link Address",
"Partition Name",
"Backup Or Not?",
"YES",
"NO",
"BIN Area Size(KB)",
"Part Number",
"USB 2.0",
"Frequency conversion(PLL)",
"Get Activation File",
"Update Mode",
"CPU and DDR2 Frequency",
"SET GPIO",
"Flash",
"System Setup",
"Import...",
"Export...",
"Row",
"Column",
"USB boot type",
"Power Off GPIO",
"BIOS Start Address",
"File system reserved partition",
"RAM Type",
"Size(M)",
"Bank",
"Row Length",
"Col Address",
"Chip Select",
"Custom",
"Chip Select0",
"Chip Select1",
"Chip Select2",
"Chip Select3",
"All",
"Initialize USB",
"Plug GPIO",
"Write Register",
"Register",
"Bit",
"Format List",
"No.",
"Partition Symbol",
"Partition Type",
"Read only",
"Hidden",
"Medium type",
"Partition Size(K)",
"Volume",
"File system Reserved partition(block)",
"Non-system Reserved partition(M)",
"SPI NAND Flash List",
"SPI NAND Flash List",
"SPI NOR Flash List",
"Start to download Infineon module",
"Failed to download Infineon module",
"Success!Devices have been Synchronized",
"Failed to boot target board",
"Start to download fls file",
"Start to download eep file",
"Failed to download fls file",
"Failed to download eep file",
"Download mode",
"AK download only",
"Infineon download only",
"Both",
"Download Related Settings",
"Baud rate",
"Download fls file",
"Download eep file",
"Browse",
"GPIO Settings",
"GPIO Setting failed",
"Failed to set parameter for producer",
"Start to download BIN",
"Failed to download BIN",
"Start to download image",
"Failed to download image",
"The drive letter of partition and image is different",
"Start to download boot",
"Failed to download boot",
"Start to write MAC address into security area",
"Failed to write MAC address into security area",
"Start to write serial number address into security area",
"Failed to write serial number address into security area",
"Begin to download frequency conversion applet",
"Failed to download frequency conversion applet",
"Download frequency conversion applet time out",
"Failed to connect USB after download frequency conversion applet",
"Set burn mode",
"Failed to set burn mode",
"Set erase mode",
"Failed to set erase mode",
"Set SPI NAND Flash parameters",
"Failed to set SPI NAND Flash parameters",
"Set security area",
"Failed to set security area",
"Failed to read back BIN file",
"Failed to get bad block information",
"Read MAC address in security area",
"Read MAC address in security area error",
"Read serial number address in security area",
"Read serial number address in security area error",
"Compare the burnt MAC address",
"Burnt MAC address exceed the maximum",
"Compare the burnt serial number address",
"Burnt serial number address exceed the maximum",
"Set reserved partition",
"Failed to set reserved partition",
"Create partition list",
"Failed to create partition list",
"Terminate burn process",
"Failed to terminate burn process",
"Please enter hex. numbers:",
"MAC Address format must be 00:00:00!",
"Word length of MAC start address high-order bit is less than 8!",
"Word length of MAC start address low-order bit is less than 8!",
"Word length of MAC end address high-order bit is less than 8!",
"Word length of MAC end address low-order bit is less than 8!",
"The string includes non-hexadecimal number!",
"The high-order bit of MAC start address is not the same as end address!",
"The low-order bit of MAC start address is bigger than end address!",
"Word length of serial number start address high-order bit is less than 32!",
"Word length of serial number start address low-order bit is less than 6!",
"Word length of serial number end address high-order bit is less than 10!",
"Word length of serial number end address low-order bit is less than 6!",
"The high-order bit of serial number start address is not the same as end address!",
"The low-order bit of serial number start address is bigger than end address!",
"Success!Current MAC address have been reset, current value equals to start value!",
"Success!Current serial number have been reset, current value equals to start value !",
"Set channel address",
"Channel address error",
"Image Create Box",
"Source folder",
"Target folder",
"Browse",
"Browse",
"Image filename",
"Capacity(MByte)",
"Page size(Byte)",
"Sector size(Byte)",
"Make information",
"Prepare for making Image ...",
"Making Image ...",
"Create",
"End",
"Success!You've made a Image.",
"Failed to make Image!",
"Getting folder info...",
"Failed to get folder info!",
"Low capacity size!",
"Configuration info error!",
"Empty source folder!",
"Empty target folder!",
"Empty image filename!",
"Empty capacity!",
"Empty sector!",
"Empty page size!",
"Failed to set SPI NAND Flash GPIO CS!",
"Failed to download channel address!",
"Failed to set com interface type!",
"Failed to download com interface type!",
"Making Image...",
"Success!You've made a Image.",
"Failed to make a Image!",
"Finished Image making and clear options!",
"Process is running, close it or not?",
"Enter the verification string",
"The file imported.",
"Failed to import a file!",
"Waiting...",
"The file exported.",
"Failed to export a file!",
"Data will be destroyed, format the device or not?",
"SPI NOR Flash Image",
"Please choose the flash:",
"SPI",
"No SPI NOR Flash to choose.",
"Failed to open help file!",
"Low-level Format",
"OK",
"Cancel",
"Volume lable name of partition should not include the following 9 words.",
"The MAC address is multicast address, please modify it.",
"At least one of the MAC address should be numbers (except 0).",
"Failed to get high ID. Please confirm if the producer version is too old.",
"Count all free block before create partition.",
"The capacity of the several NAND/SD channel is different.",
"Check the capacity size of every device.",
"Read back BIN completed.",
"Read back BIN, please enter massboot to start.",
"Read back SPI NOR Flash completed.",
"Failed to read back SPI NOR Flash!",
"Read back SPI NOR Flash, please enter massboot to start.",
"Start to read back all the SPI NOR Flash data.",
"Read OTP serial number",
"Failed to read OTP serial number",
"Write OTP serial number",
"Failed to write OTP serial number",
"OTP serial number existed",
"No file name in partition table",
"Get partition wrong when download image",
"Start to burn environmental variable data",
"Burn environmental variable data error",
"Partition name and BIN file name are different",
"Failed to download SPI NOR Flash image.",
"Only one SPI image file can be downloaded.",
"Start to download SPI image file.",
"Download SPI image file finished.",
"Erase before burning (erase by partition size and this function aims to save time by erasing 64K each time).",
"No erasing needed during burning (this function aims to save time by burning brand-new SPI without erasing).",
"Name exceeded the max value 8",
"Start to erase partition",
"Failed to erase partition",
"Failed to check file type",
"Start to get Bluetooth address",
"Bluetooth address is bigger than end address",
"Bluetooth address length error",
"Bluetooth address error",
"Failed to write Bluetooth address",
"Start to write Bluetooth address",
"The number of erased block is more than total number",
"Erase block 0",
"Failed to erase block 0",
"Set kernel position",
"Kernel position(K)",
"Microswitch(no vin_chg)",
"Check Info",
"Create U-Boot Image(&U)",
"U-Boot Image",
"Please choose the flash:",
"Offset(0x)",
"Size(0x)",
"Erasing all partition...",
"Update",
"Boot Mode",
"In non-security boot mode, burn firmware of non-security boot mode.",
"In non-security boot mode, burn firmware of security boot mode.",
"In security boot mode, burn firmware of security boot mode.",
"Download 1k signature verification data",
"Failed to download 1k signature verification data",
"Signature Data",
"Copyright",
"2001-2023 Anyka Microelectronics. All rights reserved.",
"Please refer to the instruction document of Anyka_USB_Burn_Tool.",
}
